|  |
| --- |
| 12 Hello, Non-geostationary horizon antenna gain. *Ge* = *Gmax* (see § 2.2 of the main body of this Appendix) for *G* = 32 − 25 log (φ) > −10 (refer to Annex 3 for definition of symbols). |